# do not edit this file, it will be overwritten on update

# run a command on remove events
ACTION=="remove", ENV{REMOVE_CMD}!="", RUN+="$env{REMOVE_CMD}"
ACTION=="remove", GOTO="default_end"

SUBSYSTEM=="virtio-ports", KERNEL=="vport*", ATTR{name}=="?*", SYMLINK+="virtio-ports/$attr{name}"

# select "system RTC" or just use the first one
SUBSYSTEM=="rtc", ATTR{hctosys}=="1", SYMLINK+="rtc"
SUBSYSTEM=="rtc", KERNEL=="rtc0", SYMLINK+="rtc", OPTIONS+="link_priority=-100"

SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", IMPORT{builtin}="usb_id", IMPORT{builtin}="hwdb --subsystem=usb"
ENV{MODALIAS}!="", IMPORT{builtin}="hwdb --subsystem=$env{SUBSYSTEM}"

ACTION!="add", GOTO="default_end"

SUBSYSTEM=="tty", KERNEL=="ptmx", GROUP="tty", MODE="0666"
SUBSYSTEM=="tty", KERNEL=="tty", GROUP="tty", MODE="0666"
SUBSYSTEM=="tty", KERNEL=="tty[0-9]*", GROUP="tty", MODE="0620"
SUBSYSTEM=="tty", KERNEL=="sclp_line[0-9]*", GROUP="tty", MODE="0620"
SUBSYSTEM=="tty", KERNEL=="ttysclp[0-9]*", GROUP="tty", MODE="0620"
SUBSYSTEM=="tty", KERNEL=="3270/tty[0-9]*", GROUP="tty", MODE="0620"
SUBSYSTEM=="vc", KERNEL=="vcs*|vcsa*", GROUP="tty"
KERNEL=="tty[A-Z]*[0-9]|ttymxc[0-9]*|pppox[0-9]*|ircomm[0-9]*|noz[0-9]*|rfcomm[0-9]*", GROUP="dialout"

SUBSYSTEM=="mem", KERNEL=="mem|kmem|port", GROUP="kmem", MODE="0640"

SUBSYSTEM=="input", GROUP="input"
SUBSYSTEM=="input", KERNEL=="js[0-9]*", MODE="0664"

SUBSYSTEM=="video4linux", GROUP="video"
SUBSYSTEM=="graphics", GROUP="video"
SUBSYSTEM=="drm", KERNEL!="renderD*", GROUP="video"
SUBSYSTEM=="dvb", GROUP="video"
SUBSYSTEM=="media", GROUP="video"
SUBSYSTEM=="cec", GROUP="video"

SUBSYSTEM=="drm", KERNEL=="renderD*", GROUP="render", MODE="0666"
SUBSYSTEM=="kfd", GROUP="render", MODE="0666"

SUBSYSTEM=="sound", GROUP="audio", \
  OPTIONS+="static_node=snd/seq", OPTIONS+="static_node=snd/timer"

SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", MODE="0664"

SUBSYSTEM=="firewire", ATTR{units}=="*0x00a02d:0x00010*", GROUP="video"
SUBSYSTEM=="firewire", ATTR{units}=="*0x00b09d:0x00010*", GROUP="video"
SUBSYSTEM=="firewire", ATTR{units}=="*0x00a02d:0x010001*", GROUP="video"
SUBSYSTEM=="firewire", ATTR{units}=="*0x00a02d:0x014001*", GROUP="video"

KERNEL=="parport[0-9]*", GROUP="lp"
SUBSYSTEM=="printer", KERNEL=="lp*", GROUP="lp"
SUBSYSTEM=="ppdev", GROUP="lp"
KERNEL=="lp[0-9]*", GROUP="lp"
KERNEL=="irlpt[0-9]*", GROUP="lp"
SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", ENV{ID_USB_INTERFACES}=="*:0701??:*", GROUP="lp"

SUBSYSTEM=="block", GROUP="disk"
SUBSYSTEM=="block", KERNEL=="sr[0-9]*", GROUP="cdrom"
SUBSYSTEM=="scsi_generic", SUBSYSTEMS=="scsi", ATTRS{type}=="4|5", GROUP="cdrom"
KERNEL=="sch[0-9]*", GROUP="cdrom"
KERNEL=="pktcdvd[0-9]*", GROUP="cdrom"
KERNEL=="pktcdvd", GROUP="cdrom"

SUBSYSTEM=="scsi_generic|scsi_tape", SUBSYSTEMS=="scsi", ATTRS{type}=="1|8", GROUP="tape"
SUBSYSTEM=="scsi_generic", SUBSYSTEMS=="scsi", ATTRS{type}=="0", GROUP="disk"
KERNEL=="qft[0-9]*|nqft[0-9]*|zqft[0-9]*|nzqft[0-9]*|rawqft[0-9]*|nrawqft[0-9]*", GROUP="disk"
KERNEL=="loop-control", GROUP="disk", OPTIONS+="static_node=loop-control"
KERNEL=="btrfs-control", GROUP="disk"
KERNEL=="rawctl", GROUP="disk"
SUBSYSTEM=="raw", KERNEL=="raw[0-9]*", GROUP="disk"
SUBSYSTEM=="aoe", GROUP="disk", MODE="0220"
SUBSYSTEM=="aoe", KERNEL=="err", MODE="0440"

KERNEL=="rfkill", MODE="0664"
KERNEL=="tun", MODE="0666", OPTIONS+="static_node=net/tun"

KERNEL=="fuse", MODE="0666", OPTIONS+="static_node=fuse"

# The static_node is required on s390x and ppc (they are using MODULE_ALIAS)
KERNEL=="kvm", GROUP="kvm", MODE="0666", OPTIONS+="static_node=kvm"

SUBSYSTEM=="ptp", ATTR{clock_name}=="KVM virtual PTP", SYMLINK += "ptp_kvm"

SUBSYSTEM=="ptp", ATTR{clock_name}=="hyperv", SYMLINK += "ptp_hyperv"

LABEL="default_end"
