# This file is part of systemd.
#
# Data imported from: http://www.linux-usb.org/usb.ids

usb:v*p*d*dc01*
 ID_USB_CLASS_FROM_DATABASE=Audio

usb:v*p*d*dc01dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Control Device

usb:v*p*d*dc01dsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=Streaming

usb:v*p*d*dc01dsc03*
 ID_USB_SUBCLASS_FROM_DATABASE=MIDI Streaming

usb:v*p*d*dc02*
 ID_USB_CLASS_FROM_DATABASE=Communications

usb:v*p*d*dc02dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Direct Line

usb:v*p*d*dc02dsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=Abstract (modem)

usb:v*p*d*dc02dsc02dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (v.25ter)

usb:v*p*d*dc02dsc02dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (PCCA101)

usb:v*p*d*dc02dsc02dp03*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (PCCA101 + wakeup)

usb:v*p*d*dc02dsc02dp04*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (GSM)

usb:v*p*d*dc02dsc02dp05*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (3G)

usb:v*p*d*dc02dsc02dp06*
 ID_USB_PROTOCOL_FROM_DATABASE=AT-commands (CDMA)

usb:v*p*d*dc02dsc02dpFE*
 ID_USB_PROTOCOL_FROM_DATABASE=Defined by command set descriptor

usb:v*p*d*dc02dsc02dpFF*
 ID_USB_PROTOCOL_FROM_DATABASE=Vendor Specific (MSFT RNDIS?)

usb:v*p*d*dc02dsc03*
 ID_USB_SUBCLASS_FROM_DATABASE=Telephone

usb:v*p*d*dc02dsc04*
 ID_USB_SUBCLASS_FROM_DATABASE=Multi-Channel

usb:v*p*d*dc02dsc05*
 ID_USB_SUBCLASS_FROM_DATABASE=CAPI Control

usb:v*p*d*dc02dsc06*
 ID_USB_SUBCLASS_FROM_DATABASE=Ethernet Networking

usb:v*p*d*dc02dsc07*
 ID_USB_SUBCLASS_FROM_DATABASE=ATM Networking

usb:v*p*d*dc02dsc08*
 ID_USB_SUBCLASS_FROM_DATABASE=Wireless Handset Control

usb:v*p*d*dc02dsc09*
 ID_USB_SUBCLASS_FROM_DATABASE=Device Management

usb:v*p*d*dc02dsc0A*
 ID_USB_SUBCLASS_FROM_DATABASE=Mobile Direct Line

usb:v*p*d*dc02dsc0B*
 ID_USB_SUBCLASS_FROM_DATABASE=OBEX

usb:v*p*d*dc02dsc0C*
 ID_USB_SUBCLASS_FROM_DATABASE=Ethernet Emulation

usb:v*p*d*dc02dsc0Cdp07*
 ID_USB_PROTOCOL_FROM_DATABASE=Ethernet Emulation (EEM)

usb:v*p*d*dc03*
 ID_USB_CLASS_FROM_DATABASE=Human Interface Device

usb:v*p*d*dc03dsc00dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Keyboard

usb:v*p*d*dc03dsc00dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Mouse

usb:v*p*d*dc03dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Boot Interface Subclass

usb:v*p*d*dc03dsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Keyboard

usb:v*p*d*dc03dsc01dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Mouse

usb:v*p*d*dc05*
 ID_USB_CLASS_FROM_DATABASE=Physical Interface Device

usb:v*p*d*dc06*
 ID_USB_CLASS_FROM_DATABASE=Imaging

usb:v*p*d*dc06dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Still Image Capture

usb:v*p*d*dc06dsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Picture Transfer Protocol (PIMA 15470)

usb:v*p*d*dc07*
 ID_USB_CLASS_FROM_DATABASE=Printer

usb:v*p*d*dc07dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Printer

usb:v*p*d*dc07dsc01dp00*
 ID_USB_PROTOCOL_FROM_DATABASE=Reserved/Undefined

usb:v*p*d*dc07dsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Unidirectional

usb:v*p*d*dc07dsc01dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Bidirectional

usb:v*p*d*dc07dsc01dp03*
 ID_USB_PROTOCOL_FROM_DATABASE=IEEE 1284.4 compatible bidirectional

usb:v*p*d*dc07dsc01dpFF*
 ID_USB_PROTOCOL_FROM_DATABASE=Vendor Specific

usb:v*p*d*dc08*
 ID_USB_CLASS_FROM_DATABASE=Mass Storage

usb:v*p*d*dc08dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=RBC (typically Flash)

usb:v*p*d*dc08dsc01dp00*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk/Interrupt

usb:v*p*d*dc08dsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk

usb:v*p*d*dc08dsc01dp50*
 ID_USB_PROTOCOL_FROM_DATABASE=Bulk-Only

usb:v*p*d*dc08dsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=SFF-8020i, MMC-2 (ATAPI)

usb:v*p*d*dc08dsc03*
 ID_USB_SUBCLASS_FROM_DATABASE=QIC-157

usb:v*p*d*dc08dsc04*
 ID_USB_SUBCLASS_FROM_DATABASE=Floppy (UFI)

usb:v*p*d*dc08dsc04dp00*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk/Interrupt

usb:v*p*d*dc08dsc04dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk

usb:v*p*d*dc08dsc04dp50*
 ID_USB_PROTOCOL_FROM_DATABASE=Bulk-Only

usb:v*p*d*dc08dsc05*
 ID_USB_SUBCLASS_FROM_DATABASE=SFF-8070i

usb:v*p*d*dc08dsc06*
 ID_USB_SUBCLASS_FROM_DATABASE=SCSI

usb:v*p*d*dc08dsc06dp00*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk/Interrupt

usb:v*p*d*dc08dsc06dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Control/Bulk

usb:v*p*d*dc08dsc06dp50*
 ID_USB_PROTOCOL_FROM_DATABASE=Bulk-Only

usb:v*p*d*dc09*
 ID_USB_CLASS_FROM_DATABASE=Hub

usb:v*p*d*dc09dsc00dp00*
 ID_USB_PROTOCOL_FROM_DATABASE=Full speed (or root) hub

usb:v*p*d*dc09dsc00dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Single TT

usb:v*p*d*dc09dsc00dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=TT per port

usb:v*p*d*dc0A*
 ID_USB_CLASS_FROM_DATABASE=CDC Data

usb:v*p*d*dc0Adsc00dp30*
 ID_USB_PROTOCOL_FROM_DATABASE=I.430 ISDN BRI

usb:v*p*d*dc0Adsc00dp31*
 ID_USB_PROTOCOL_FROM_DATABASE=HDLC

usb:v*p*d*dc0Adsc00dp32*
 ID_USB_PROTOCOL_FROM_DATABASE=Transparent

usb:v*p*d*dc0Adsc00dp50*
 ID_USB_PROTOCOL_FROM_DATABASE=Q.921M

usb:v*p*d*dc0Adsc00dp51*
 ID_USB_PROTOCOL_FROM_DATABASE=Q.921

usb:v*p*d*dc0Adsc00dp52*
 ID_USB_PROTOCOL_FROM_DATABASE=Q.921TM

usb:v*p*d*dc0Adsc00dp90*
 ID_USB_PROTOCOL_FROM_DATABASE=V.42bis

usb:v*p*d*dc0Adsc00dp91*
 ID_USB_PROTOCOL_FROM_DATABASE=Q.932 EuroISDN

usb:v*p*d*dc0Adsc00dp92*
 ID_USB_PROTOCOL_FROM_DATABASE=V.120 V.24 rate ISDN

usb:v*p*d*dc0Adsc00dp93*
 ID_USB_PROTOCOL_FROM_DATABASE=CAPI 2.0

usb:v*p*d*dc0Adsc00dpFD*
 ID_USB_PROTOCOL_FROM_DATABASE=Host Based Driver

usb:v*p*d*dc0Adsc00dpFE*
 ID_USB_PROTOCOL_FROM_DATABASE=CDC PUF

usb:v*p*d*dc0Adsc00dpFF*
 ID_USB_PROTOCOL_FROM_DATABASE=Vendor specific

usb:v*p*d*dc0B*
 ID_USB_CLASS_FROM_DATABASE=Chip/SmartCard

usb:v*p*d*dc0D*
 ID_USB_CLASS_FROM_DATABASE=Content Security

usb:v*p*d*dc0E*
 ID_USB_CLASS_FROM_DATABASE=Video

usb:v*p*d*dc0Edsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Video Control

usb:v*p*d*dc0Edsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=Video Streaming

usb:v*p*d*dc0Edsc03*
 ID_USB_SUBCLASS_FROM_DATABASE=Video Interface Collection

usb:v*p*d*dc58*
 ID_USB_CLASS_FROM_DATABASE=Xbox

usb:v*p*d*dc58dsc42*
 ID_USB_SUBCLASS_FROM_DATABASE=Controller

usb:v*p*d*dcDC*
 ID_USB_CLASS_FROM_DATABASE=Diagnostic

usb:v*p*d*dcDCdsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Reprogrammable Diagnostics

usb:v*p*d*dcDCdsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=USB2 Compliance

usb:v*p*d*dcE0*
 ID_USB_CLASS_FROM_DATABASE=Wireless

usb:v*p*d*dcE0dsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Radio Frequency

usb:v*p*d*dcE0dsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Bluetooth

usb:v*p*d*dcE0dsc01dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Ultra WideBand Radio Control

usb:v*p*d*dcE0dsc01dp03*
 ID_USB_PROTOCOL_FROM_DATABASE=RNDIS

usb:v*p*d*dcE0dsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=Wireless USB Wire Adapter

usb:v*p*d*dcE0dsc02dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Host Wire Adapter Control/Data Streaming

usb:v*p*d*dcE0dsc02dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Device Wire Adapter Control/Data Streaming

usb:v*p*d*dcE0dsc02dp03*
 ID_USB_PROTOCOL_FROM_DATABASE=Device Wire Adapter Isochronous Streaming

usb:v*p*d*dcEF*
 ID_USB_CLASS_FROM_DATABASE=Miscellaneous Device

usb:v*p*d*dcEFdsc01dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Microsoft ActiveSync

usb:v*p*d*dcEFdsc01dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Palm Sync

usb:v*p*d*dcEFdsc02dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Interface Association

usb:v*p*d*dcEFdsc02dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=Wire Adapter Multifunction Peripheral

usb:v*p*d*dcEFdsc03dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=Cable Based Association

usb:v*p*d*dcEFdsc05*
 ID_USB_SUBCLASS_FROM_DATABASE=USB3 Vision

usb:v*p*d*dcFE*
 ID_USB_CLASS_FROM_DATABASE=Application Specific Interface

usb:v*p*d*dcFEdsc01*
 ID_USB_SUBCLASS_FROM_DATABASE=Device Firmware Update

usb:v*p*d*dcFEdsc02*
 ID_USB_SUBCLASS_FROM_DATABASE=IRDA Bridge

usb:v*p*d*dcFEdsc03*
 ID_USB_SUBCLASS_FROM_DATABASE=Test and Measurement

usb:v*p*d*dcFEdsc03dp01*
 ID_USB_PROTOCOL_FROM_DATABASE=TMC

usb:v*p*d*dcFEdsc03dp02*
 ID_USB_PROTOCOL_FROM_DATABASE=USB488

usb:v*p*d*dcFF*
 ID_USB_CLASS_FROM_DATABASE=Vendor Specific Class

usb:v*p*d*dcFFdscFF*
 ID_USB_SUBCLASS_FROM_DATABASE=Vendor Specific Subclass

usb:v*p*d*dcFFdscFFdpFF*
 ID_USB_PROTOCOL_FROM_DATABASE=Vendor Specific Protocol
