# SCSI-ID mappings for sg3_utils

ACTION=="remove", GOTO="sg3_utils_id_end"

SUBSYSTEM!="block", GOTO="sg3_utils_id_end"

# Import values for partitions
ENV{DEVTYPE}=="partition", IMPORT{parent}="SCSI_*", ENV{ID_SCSI}="1"
# SCSI INQUIRY values
# If the 'inquiry' sysfs attribute is present the kernel will already
# have scanned for VPD pages, so if the vpd page attribute is not
# present it is not supported (or deemed unsafe to access).
# Hence we can skip the call to sg_inq and avoid I/O altogether.
# Set 'ID_SCSI_INQUIRY=0' in an earlier udev rule if the kernel
# fails to scan VPD pages correctly; the rules will then fall
# back to calling sg_vpd directly.
KERNEL=="sd*[!0-9]|sr*", ENV{ID_SCSI_INQUIRY}!="?*", IMPORT{program}="/usr/bin/sg_inq --export --inhex=/sys/block/$kernel/device/inquiry --raw", ENV{ID_SCSI}="1", ENV{ID_SCSI_INQUIRY}="1"
KERNEL=="sd*[!0-9]|sr*", ENV{ID_SCSI}!="1", IMPORT{program}="/usr/bin/sg_inq --export $tempnode", ENV{ID_SCSI}="1"
# scsi_id compat mappings
ENV{SCSI_VENDOR}=="?*", ENV{ID_VENDOR}="$env{SCSI_VENDOR}"
ENV{SCSI_VENDOR_ENC}=="?*", ENV{ID_VENDOR_ENC}="$env{SCSI_VENDOR_ENC}"
ENV{SCSI_MODEL}=="?*", ENV{ID_MODEL}="$env{SCSI_MODEL}"
ENV{SCSI_MODEL_ENC}=="?*", ENV{ID_MODEL_ENC}="$env{SCSI_MODEL_ENC}"
ENV{SCSI_REVISION}=="?*", ENV{ID_REVISION}="$env{SCSI_REVISION}"
ENV{SCSI_TYPE}=="?*", ENV{ID_TYPE}="$env{SCSI_TYPE}"
# SCSI EVPD page 0x80 values
KERNEL=="sd*[!0-9]|sr*", ENV{ID_SCSI}=="1", ENV{ID_SCSI_INQUIRY}=="1", IMPORT{program}="/usr/bin/sg_inq --export --inhex=/sys/block/$kernel/device/vpd_pg80 --raw"
KERNEL=="sd*[!0-9]|sr*", ENV{ID_SCSI}=="1", ENV{ID_SCSI_INQUIRY}!="1", IMPORT{program}="/usr/bin/sg_inq --export --page=sn $tempnode"
# SCSI EVPD page 0x83 values
KERNEL=="sd*[!0-9]", ENV{ID_SCSI}=="1", ENV{ID_SCSI_INQUIRY}=="1", IMPORT{program}="/usr/bin/sg_inq --export --inhex=/sys/block/$kernel/device/vpd_pg83 --raw"
KERNEL=="sd*[!0-9]|sr*", ENV{ID_SCSI}=="1", ENV{ID_SCSI_INQUIRY}!="1", IMPORT{program}="/usr/bin/sg_inq --export --page=di $tempnode"

# ID_WWN compat mapping
ENV{SCSI_IDENT_LUN_NAA_REGEXT}=="?*", ENV{ID_WWN}!="?*", ENV{ID_WWN}="0x$env{SCSI_IDENT_LUN_NAA_REGEXT}"
ENV{SCSI_IDENT_LUN_NAA_REG}=="?*", ENV{ID_WWN}!="?*", ENV{ID_WWN}="0x$env{SCSI_IDENT_LUN_NAA_REG}"
ENV{SCSI_IDENT_LUN_NAA_EXT}=="?*", ENV{ID_WWN}!="?*", ENV{ID_WWN}="0x$env{SCSI_IDENT_LUN_NAA_EXT}"
ENV{SCSI_IDENT_LUN_NAA_LOCAL}=="?*", ENV{ID_WWN}!="?*", ENV{ID_WWN}="0x$env{SCSI_IDENT_LUN_NAA_LOCAL}"
ENV{SCSI_IDENT_LUN_NAA_REGEXT}=="?*", ENV{ID_WWN_WITH_EXTENSION}!="?*", ENV{ID_WWN_WITH_EXTENSION}="0x$env{SCSI_IDENT_LUN_NAA_REGEXT}"
ENV{SCSI_IDENT_LUN_NAA_EXT}=="?*", ENV{ID_WWN_WITH_EXTENSION}!="?*", ENV{ID_WWN_WITH_EXTENSION}="0x$env{SCSI_IDENT_LUN_NAA_EXT}"
ENV{ID_WWN}=="?*", ENV{ID_WWN_WITH_EXTENSION}!="?*", ENV{ID_WWN_WITH_EXTENSION}="$env{ID_WWN}"

# ata_id compability
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_ATA}=="?*", ENV{ID_BUS}="ata", ENV{ID_ATA}="1", ENV{ID_SERIAL}="$env{SCSI_IDENT_LUN_ATA}"
ENV{ID_SERIAL_SHORT}!="?*", ENV{SCSI_VENDOR}=="ATA", ENV{SCSI_IDENT_LUN_VENDOR}=="?*", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_VENDOR}"
# Compat ID_SERIAL setting
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_NAA_REGEXT}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="3$env{SCSI_IDENT_LUN_NAA_REGEXT}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_NAA_REGEXT}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_NAA_REG}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="3$env{SCSI_IDENT_LUN_NAA_REG}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_NAA_REG}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_NAA_EXT}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="3$env{SCSI_IDENT_LUN_NAA}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_NAA_EXT}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_EUI64}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="2$env{SCSI_IDENT_LUN_EUI64}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_EUI64}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_NAME}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="8$env{SCSI_IDENT_LUN_NAME}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_NAME}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_T10}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="1$env{SCSI_IDENT_LUN_T10}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_T10}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_NAA_LOCAL}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="3$env{SCSI_IDENT_LUN_NAA_LOCAL}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_NAA_LOCAL}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_LUN_VENDOR}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="0$env{SCSI_VENDOR}_$env{SCSI_MODEL}_$env{SCSI_IDENT_LUN_VENDOR}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_LUN_VENDOR}"
ENV{ID_SERIAL}!="?*", ENV{SCSI_IDENT_SERIAL}=="?*", ENV{ID_BUS}="scsi", ENV{ID_SERIAL}="S$env{SCSI_VENDOR}_$env{SCSI_MODEL}_$env{SCSI_IDENT_SERIAL}", ENV{ID_SERIAL_SHORT}="$env{SCSI_IDENT_SERIAL}"
LABEL="sg3_utils_id_end"
