# This file is part of systemd.
#
# The lookup keys are composed in:
#   60-sensor.rules
#
# Note: The format of the "sensor:" prefix match key is a contract between the
# rules file and the hardware data, it might change in later revisions to
# support more or better matches, it is not necessarily expected to be a stable
# ABI.
#
# Match string formats:
# sensor:modalias:<parent modalias pattern>:dmi:<dmi pattern>
#
# The device modalias can be seen in the `modalias` file of the sensor parent,
# for example:
#   cat /sys/`udevadm info -q path -n /dev/iio:device0`/../modalias
#
# The full DMI string of the running machine can be read from
#   /sys/class/dmi/id/modalias
# That requires a kernel built with CONFIG_DMIID set, which is common.
# The full DMI string is not needed here and the meaning of individual parts
# can be seen in the source of the DMIID kernel module
#   https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/tree/drivers/firmware/dmi-id.c
#
# To add local entries, create a new file
#   /etc/udev/hwdb.d/61-sensor-local.hwdb
# and add your rules there. To load the new rules execute (as root):
#   systemd-hwdb update
#   udevadm trigger -v -p DEVNAME=/dev/iio:deviceXXX
# where /dev/iio:deviceXXX is the device in question.
#
# If your changes are generally applicable, preferably send them as a pull
# request to
#   https://github.com/systemd/systemd
# or create a bug report on https://github.com/systemd/systemd/issues and
# include your new rules, a description of the device, and the output of
#   udevadm info --export-db
#
# For hwdb format and systemd behavior:
#   https://www.freedesktop.org/software/systemd/man/hwdb.html
#
# Allowed properties are:
#    ACCEL_MOUNT_MATRIX=<matrix>
#    PROXIMITY_NEAR_LEVEL=<value>
#
# where <matrix> is a mount-matrix in the format specified in the IIO
# subsystem[1]. The default, when unset, is equivalent to:
#   ACCEL_MOUNT_MATRIX=1, 0, 0; 0, 1, 0; 0, 0, 1
# eg. the identity matrix,
# and <value> is an integer value above which an object is considered
# close by a proximity sensor:
#   PROXIMITY_NEAR_LEVEL=100
#
# [1]: https://git.kernel.org/cgit/linux/kernel/git/torvalds/linux.git/commit/?id=dfc57732ad38f93ae6232a3b4e64fd077383a0f1
#
# Note for devices where the display (LCD panel) is mounted non upright
# in the device's casing, e.g. mounted upside-down or 90 degree rotated,
# the ACCEL_MOUNT_MATRIX should be such that the x and y axis matches the
# x and y axis of the display, not those of the casing, so that desktop
# environments using the accelerometer data for rotation will e.g.
# automatically flip their output for an upside-down display when the device
# is held upright.
#
#    ACCEL_LOCATION=<location>
#
# where <location> is the location of the sensor. This value could be 'base'
# or 'display'. The default, when unset, is equivalent to:
#    ACCEL_LOCATION=display
#
# A note about setting ACCEL_MOUNT_MATRIX for ACCEL_LOCATION=base sensors,
# on 360 degree hinges style 2-in-1s with 2 sensors (one in the display and
# 1 in the base). Userspace will use both sensors to calculate the angle between
# the 2 halves and the angle is defined as being 0 when the device is folded
# as a regular clamshell laptop with its lid closed. This means that the
# base-accelerometer's mount-matrix must be such, that after applying
# the mount-matrices to both sensors, the base-accelerometer's readings must
# be identical to the display-accelerometer's readings (when the lid is
# closed).
#
# Sort by brand, model

#########################################
# Acer
#########################################
sensor:modalias:acpi:KIOX0009*:dmi:*:svnAcer:pnAspireSW3-016:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, -1

sensor:modalias:acpi:INVN6500*:dmi:*svn*Acer*:*pn*AspireSW5-011:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svn*Acer*:*pn*AspireSW5-012:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

sensor:modalias:acpi:BOSC0200*:dmi:*svnAcer*:*TP-SW5-017-17BU:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, -1

sensor:modalias:acpi:BMA250E*:dmi:*:svnAcer:pnIconiaW1-810:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

sensor:modalias:acpi:SMO8500:*:dmi:*Acer*:pnOneS1002:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, -1

sensor:modalias:acpi:KIOX0009*:dmi:*:svnAcer:pnOneS1003:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

sensor:modalias:acpi:BOSC0200*:dmi:*:svnAcer*:pnSwitchSW312-31:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:BOSC0200*:dmi:*svn*Acer*:*pn*Spin*SP111-32:*
sensor:modalias:acpi:BOSC0200*:dmi:*svn*Acer*:*pn*Spin*SP111-33:*
sensor:modalias:acpi:BOSC0200*:dmi:*svnAcer*:*pnSpinSP111-34:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Archos
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnARCHOS:pnARCHOS80Cesium:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# AsusTek
#########################################
sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:*pnT100CHI:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:pnT300CHI:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:*pnM80TA:*
sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:*pnT100TA:*
sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:pnT200TA:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:*pnTP201SA:*
sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:pn*E205SA:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svn*ASUSTeK*:*pn*TP300LA:*
sensor:modalias:acpi:INVN6500*:dmi:*svn*ASUSTeK*:*pn*TP300LD:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

sensor:modalias:acpi:INVN6500*:dmi:*svnASUSTeK*:*pn*Q551LN:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:KXJ2109*:dmi:*:svnASUSTeK*:pnME176C:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP300LJ:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP500LAB:*
sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP500LB:*
sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP550LA:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP300LD:*
sensor:modalias:acpi:SMO8500*:dmi:*svn*ASUSTeK*:*pn*TP300LAB:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:BOSC0200*:dmi:*svn*ASUSTeK*:*pn*TP412UA:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Axxo
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnStandard:pnWCBT1011::*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Chuwi
#########################################

# Chuwi Vi8 (CWI506)
sensor:modalias:acpi:BMA250E*:dmi:bvnINSYDECorp.:bvrCHUWI.D86JLBNR*:svnInsyde:pni86:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Vi8 Plus (CWI519)
sensor:modalias:acpi:BOSC0200*:dmi:*:svnHampoo:pnD2D3_Vi8A1:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Vi10 (CWI505)
sensor:modalias:acpi:BMA250E*:dmi:bvnINSYDECorp.:bvrG1D_S165*:svnilife:pnS165:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Chuwi Hi8 (CWI509)
sensor:modalias:acpi:BMA250E*:dmi:*svnilife*:pnS806:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Chuwi Hi8 Pro (CWI513)
sensor:modalias:acpi:BOSC0200*:dmi:*:svnHampoo:pnX1D3_C806N:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Hi10 (CWI515)
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:*:svnDefaultstring:pnDefaultstring:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Hi10 (CWI1515)
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvrP02A_C106.60E:*:svnDefaultstring:pnDefaultstring:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Hi10 Pro
sensor:modalias:acpi:BOSC0200*:dmi:*:svn*CHUWIINNOVATIONANDTECHNOLOGY*:pnHi10protablet:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Chuwi Hi10 X
sensor:modalias:acpi:MXC6655*:dmi:*:svnCHUWIInnovationAndTechnology*:pnHi10X:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Chuwi Hi12
sensor:modalias:acpi:BOSC0200*:dmi:*:svnHampoo:pnP02BD6_HI-122LP:*
sensor:modalias:acpi:BOSC0200*:dmi:*:svnDefaultstring:pnDefaultstring:*
sensor:modalias:acpi:BOSC0200*:dmi:*:svnHampoo:pnE4D6_HI-122LP:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Chuwi Hi13
sensor:modalias:acpi:KIOX000A*:dmi:*:svnChuwi*:pnHi13:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Chuwi Hi13 (CWI534) with BMA250 sensor
# Note this sets the norm matrix, since the matrix which the kernel reads
# from the ACPI tables is actually wrong on these models
sensor:modalias:acpi:BOSC0200*:dmi:*:svnChuwi*:pnHi13:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, 1, 0; 0, 0, 1

# Chuwi HiBook
# Chuwi HiBook does not have its product name filled, so we
# match the entire dmi-alias, assuming that the use of a BOSC0200 +
# bios-version + bios-date combo is unique
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd05/07/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnHampoo:rnCherryTrailCR:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd05/28/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnHampoo:rnCherryTrailCR:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Chuwi HiBook Pro (CWI526)
sensor:modalias:acpi:BOSC0200*:dmi:*:svnHampoo*:pnP1D6_C109K:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Chuwi CoreBook
# Chuwi CoreBook does not have its product name filled, so we
# match the entire dmi-alias
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvrY13D_KB133.103:bd06/01/2018:svnHampoo:pnDefaultstring:pvrV100:rvnHampoo:rnY13D_KB133:rvrV100:cvnDefaultstring:ct9:cvrDefaultstring:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Connect
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*:svnConnect:pnTablet9:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Cube
#########################################

# Cube iWork8 Air
sensor:modalias:acpi:KIOX000A*:dmi:*:svncube:pni1-TF:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Cube i7
sensor:modalias:acpi:SMO8500*:dmi:*:svncube:pni7:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Cube i7 Stylus, i7 Stylus I8L Model, i7 Book (i16) and Mix Plus (i18B)
sensor:modalias:acpi:KIOX000A*:dmi:*:svnCube:pni7Stylus:*
sensor:modalias:acpi:KIOX000A*:dmi:*:svnCube:pni8-L:*
sensor:modalias:acpi:KIOX000A*:dmi:*:svnCube:pni16:*
sensor:modalias:acpi:KIOX000A*:dmi:*:svnCube:pni18B:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# Cube iWork 10 Flagship
sensor:modalias:acpi:BOSC0200*:dmi:*:svnCube:pnI15-TC:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Cube iWork 11 Stylus
sensor:modalias:acpi:KIOX000A*:dmi:*:svncube:pni8-T:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Cube KNote 5
sensor:modalias:acpi:KIOX000A*:dmi:*:svnALLDOCUBE:pni1102:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Cytrix (Mytrix)
#########################################
sensor:modalias:acpi:*KIOX000A*:dmi:*svn*CytrixTechnology:*pn*Complex11t:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Dell
#########################################
sensor:modalias:platform:HID-SENSOR-200073:dmi:*svnDell*:pnVostro5581:*
 ACCEL_LOCATION=base

sensor:modalias:platform:HID-SENSOR-200073:dmi:*svnDell*:sku0A3E:*
 ACCEL_LOCATION=base

sensor:modalias:platform:HID-SENSOR-200073:dmi:*svnDell*:sku0B0B:*
 ACCEL_LOCATION=base

# Dell Venue 8 Pro 3845
sensor:modalias:acpi:INVN6500*:dmi:*svnDellInc.*:pnVenue8Pro3845:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Dell Venue 10 Pro 5055
sensor:modalias:acpi:INVN6500*:dmi:*svnDell*:pnVenue10Pro5055:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, 1

#########################################
# DEXP
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*svn*DEXP*:*pn*DEXPOEM:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Digibras
#########################################

# Digibras F10-30
sensor:modalias:acpi:SMO8500*:dmi:*:svnDigibras:pnF10-30:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# DIGMA
#########################################

# Digma CITI E203
sensor:modalias:acpi:BOSC0200*:dmi:*:svnDigma:pnCITIE203ES2010EW:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Endless
#########################################
sensor:modalias:acpi:ACCE0001*:dmi:*svnEndless*:*pnELT-NL3:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 0, 0, -1; -1, 0, 0

#########################################
# Estar
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnEstar:pneSTARBEAUTYHDIntelQuadcore:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Eve Technology
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*:svnEVE*:pnEveV:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Geo Computers
#########################################

# Geoflex
sensor:modalias:acpi:KIOX010A*:dmi:*:svnGEO*:pnGeoFlex*:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Glavey
#########################################

# Glavey TM800A550L
sensor:modalias:acpi:KXCJ9000*:dmi:*:bvrZY-8-BI-PX4S70VTR400-X423B-005-D:*:rvnAMICorporation:rnAptioCRB:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Google Chromebooks
#########################################
sensor:modalias:platform:cros-ec-accel:dmi:*:svnGOOGLE:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1

# caroline board (Samsung Chromebook Pro) reports itself as svnGoogle
sensor:modalias:platform:cros-ec-accel:dmi:*:svnGoogle:pnCaroline*:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1

# Dell Inspiron Chromebook 14 2-in-1
sensor:modalias:platform:cros-ec-accel:dmi:*svnGoogle:pnVayne*:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1

# nocturne board (Google Pixel Slate)
sensor:modalias:platform:cros-ec-accel:dmi:*Google_Nocturne*:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# GP-electronic
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:bvnINSYDECorp.:bvrBYT70A.YNCHENG.WIN.007:*:svnInsyde:pnT701:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# GPD
#########################################

# GPD win (version 1, with the X5-Z8750 CPU)
# Note we match all dmi fields including the BIOS date checking for all known
# BIOS dates, since the strings are unfortunately very generic.
# Out of a sample set of 15 similar boards only the GPDwin has board_vendor=AMI
# and no other devices have both board_name *and* product_name set to
# "Default string". So combined with the sensor modalias and BIOS date this
# should be unique enough to identify the GPDwin
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd10/25/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd11/18/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd12/23/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd12/26/2016:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd02/21/2017:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd03/20/2017:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.11:bd05/25/2017:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnAMICorporation:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
 ACCEL_LOCATION=base

#########################################
# HP
#########################################

# Most HP Laptop using the lis3lv02d device have it in the base,
# mark these sensors as such.
sensor:modalias:platform:lis3lv02d:dmi:*svn*Hewlett-Packard*:*
sensor:modalias:platform:lis3lv02d:dmi:*svn*HP*:*
 ACCEL_LOCATION=base

sensor:modalias:acpi:SMO8500*:dmi:*:svnHewlett-Packard:pnHPStream7Tablet:*
sensor:modalias:acpi:SMO8500*:dmi:*:svnHewlett-Packard:pnHPStream8Tablet:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# HP Pavillion X2 10-n000nd
sensor:modalias:i2c:bmc150_accel:dmi:*:svnHewlett-Packard:pnHPPavilionx2Detachable:*:rn815D:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# I.T.Works
#########################################

# The I.T.Works TW891 2-in-1's DMI has the product-name field set, but not
# the sys-vendor field. This makes the DMI data a bit generic, so we match
# the whole dmi modalias, except for the BIOS version/date
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:*:svnTobefilledbyO.E.M.:pnTW891:pvrTobefilledbyO.E.M.:rvnTobefilledbyO.E.M.:rnTW891:rvr1.0:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# I.T.Works TW701 7" windows tablet, same hw as Trekstor ST70416-6
sensor:modalias:acpi:BMA250*:dmi:*:bvritWORKS.G.WI71C.JGBMRB*:*:svnInsyde:pni71c:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Irbis
#########################################

#TW90
sensor:modalias:acpi:BOSC0200*:dmi:*:svnIRBIS:pnTW90:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, 1

# NB111
sensor:modalias:acpi:KIOX010A*:dmi:*svn*IRBIS*:*pn*NB111:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#TW118
sensor:modalias:acpi:BOSC0200*:dmi:*:svnIRBIS:pnTW118:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# iOTA 360
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*svn*iOTA*:*pn*IOTA2210:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Jumper
#########################################

# EZpad mini 3
sensor:modalias:acpi:BOSC0200*:dmi:bvnINSYDECorp.:bvrjumperx.T87.KFBNEE:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# EZpad 6 Pro
sensor:modalias:acpi:BOSC0200*:dmi:*:svnJumper:pnEZpad:*:rvr.A006:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, 1

# EZpad 7
sensor:modalias:acpi:KIOX0009*:dmi:*:bvrJumper12x.WJ2012.bsBKRCP*:svnJumper:pnEZpad:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# EZpad Go
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:*:svnjumper:pnEZpad:*:ct31:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Kazam
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:bvnINSYDECorp.:bvrVISION.I22K*:svnKAZAM:pnVISION:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# KD / Kurio
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnKDInteractive:pnKurioSmart:*:rnKDM960BCP:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Lamina
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*svnLamina*:*pnT701BR.SE:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

sensor:modalias:acpi:KIOX000A*:dmi:*svnLAMINA:pnT-1016BNORD:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Lenovo
#########################################
sensor:modalias:acpi:NCPE0388*:dmi:*:rnLenovoYOGA510-14IKB:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, 1

sensor:modalias:acpi:BOSC0200*:dmi:*ThinkPadYoga11e3rdGen:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, -1

sensor:modalias:acpi:BOSC0200*:dmi:*:svnLENOVO:*pvrThinkPadYoga11e4thGen:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, -1

# Miix3-1030
sensor:modalias:acpi:BMA250E*:dmi:bvnLENOVO:*:pvrLenovoMIIX3-1030:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Miix3-830
sensor:modalias:acpi:SMO8500*:dmi:bvnLENOVO:*:pvrLenovoMIIX3-830:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# IdeaPad D330-10IGM (both 81H3 and 81MD product names)
sensor:modalias:acpi:BOSC0200*:dmi:*:svnLENOVO:*:pvrLenovoideapadD330-10IGM:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; -1, 0, 0; 0, 0, 1

# IdeaPad Miix 300
sensor:modalias:acpi:SMO8500*:dmi:bvnLENOVO:*:pvrMIIX300-*:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# IdeaPad Miix 310 note this only is for BIOS version (bvr) 1HCN4?WW and 1HCN2?WW, which has
# a portrait LCD panel, versions with bvr 1HCN3?WW have a landscape panel
sensor:modalias:acpi:KIOX000A*:dmi:bvnLENOVO:bvr1HCN4?WW:*:svnLENOVO:pn80SG:*
sensor:modalias:acpi:KIOX000A*:dmi:bvnLENOVO:bvr1HCN2?WW:*:svnLENOVO:pn80SG:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# IdeaPad Miix 320, different batches use a different sensor
sensor:modalias:acpi:*BOSC0200*:dmi:*:svnLENOVO*:pn80XF:*
sensor:modalias:acpi:SMO8840*:dmi:*:svnLENOVO:pn80XF:pvrLenovoMIIX320:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# IdeaPad Miix 510, multiple expressions match different internal names
# pn80U1 matches IdeaPad Miix510-12ISK
sensor:modalias:acpi:*BOSC0200*:dmi:*:svnLENOVO*:pn80XE:*
sensor:modalias:acpi:*BOSC0200*:dmi:*:svnLENOVO*:pn80U1:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Yoga 300-11IBR, display sensor
sensor:modalias:acpi:DUAL250E*:dmi:*:svnLENOVO:*:pvrLenovoYoga300-11IBR:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1
 ACCEL_LOCATION=display

# Yoga 300-11IBR, base sensor
sensor:modalias:i2c:bmc150_accel:dmi:*:svnLENOVO:*:pvrLenovoYoga300-11IBR:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, 1, 0; 0, 0, -1
 ACCEL_LOCATION=base

#########################################
# LINX
#########################################

# Linx 1010B
sensor:modalias:acpi:BOSC0200*:dmi:*:svnLINX*:pnLINX1010B:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, -1

# Linx 12X64, 12V64 and Vision 8
sensor:modalias:acpi:KIOX000A*:dmi:*:svnLINX*:pnLINX12*64:*
sensor:modalias:acpi:KIOX000A*:dmi:*:svnLINX:pnVISION004:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Mediacom
#########################################
# Mediacom Winpad 7.0 W700
sensor:modalias:acpi:BMA250*:dmi:*svnMEDIACOM*:pnWinPad7W10-WPW700:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Medion
#########################################
# Medion Akoya E2228T MD61900
sensor:modalias:acpi:KIOX020A*:dmi:*:svnMEDION:pnE2228TMD61900:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1
 ACCEL_LOCATION=base

# Medion Akoya E1239T MD60568
sensor:modalias:acpi:KIOX0009*:dmi:*:svnMEDION:pnE1239TMD60568:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Medion Akoya E2212T MD99720
sensor:modalias:acpi:SMO8500*:dmi:*:svnMEDION:pnAkoyaE2212TMD99720:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# Medion Akoya E2215T MD60198
sensor:modalias:acpi:KIOX000A*:dmi:*svnMEDION:pnE2215TMD60198:*
# Medion Akoya E3216 MD60900
# Medion Akoya E3221 MD61237
# Medion Akoya E2292 MD63390
# Medion Akoya E2293 MD61130
# Medion Akoya E2293 MD61144
# Medion Akoya E3222 MD62450
# and presumably all other Akoya Exxxx
sensor:modalias:acpi:KIOX010A*:dmi:*:svnMEDION:pnE*:*
# Medion Akoya E3222 MD62450
sensor:modalias:acpi:KIOX010A*:dmi:*:svnMEDION:pnMEDION*:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1
 ACCEL_LOCATION=display

# Same as above, but for base sensor
sensor:modalias:acpi:KIOX020A*:dmi:*:svnMEDION:pnE*:*
sensor:modalias:acpi:KIOX020A*:dmi:*:svnMEDION:pnMEDION*:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, -1
 ACCEL_LOCATION=base

#########################################
# MPMAN
#########################################

# MPMAN Converter 9, same hw as the I.T.Works TW891 2-in-1
sensor:modalias:acpi:SMO8500*:dmi:*:svnMPMAN:pnConverter9:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# MPMAN MPWIN895C
sensor:modalias:acpi:BMA250E*:dmi:*:svnMPMAN:pnMPWIN8900CL:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# MSI
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnMicro-StarInternationalCo.,Ltd.:pnS100:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, 1

#########################################
# MYRIA
#########################################

# MY8307
sensor:modalias:acpi:BOSC0200*:dmi:*:svnCompletElectroServ:pnMY8307:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# MY8312
sensor:modalias:acpi:KIOX010A*:dmi:*:svnCompletElectroServSA:pnMY8312:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Nuvision (TMax)
#########################################

# Nuvision/TMAX 8" Windows signature edition. TM800W560L
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTMAX:pnTM800W560L:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Nuvision Solo 10 Draw. TM101W610L
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTMAX:pnTM101W610L:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Nuvision Encite Split 11. NES11-C432SSA
sensor:modalias:acpi:BOSC0200*:dmi:*:svnNuvision:pnNES11:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Odys
#########################################
sensor:modalias:acpi:BOSC0200*:dmi:bvnINSYDECorp.:bvrODYS.FUSIONWIN12:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Onda
#########################################
sensor:modalias:acpi:BOSC0200*:dmi:*:svnONDA:pnV80PLUS:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:BMA250E*:dmi:bvnINSYDECorp.:bvrONDA.D89*:svnInsyde:pnONDATablet:*
sensor:modalias:acpi:BMA250E*:dmi:bvnINSYDECorp.:bvrONDA.D86*:svnONDA:pnV820wDualOS:*
sensor:modalias:acpi:BMA250E*:dmi:bvnINSYDECorp.:bvrONDA.W89*:svnInsyde:pnONDATablet:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Onda v975w, generic DMI strings, match entire dmi modalias inc. bios-date
sensor:modalias:acpi:SMO8500*:dmi:bvnAmericanMegatrendsInc.:bvr5.6.5:bd07/25/2014:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnAptioCRB:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# One-netbook
#########################################

# One-netbook OneMix 2s
# OneMix 2s has no product name filled, matching entire dmi-alias
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvr5.12:bd10/26/2018:br5.12:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnDefaultstring:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# One-netbook OneMix 3 Pro
sensor:modalias:acpi:BOSC0200*:dmi:*svnONE-NETBOOKTECHNOLOGYCO*:pnOne-Mix3Pro:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

# One-netbook OneMix 3s
# OneMix 3s has no product name filled, matching entire dmi-alias
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvr5.12:bd07/17/2019:br5.12:svnDefaultstring:pnDefaultstring:pvrDefaultstring:rvnDefaultstring:rnDefaultstring:rvrDefaultstring:cvnDefaultstring:ct3:cvrDefaultstring:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Peaq
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnPEAQ:pnPEAQPMMC1010MD99187:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Pipo
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*:svnPIPO:pnW2S:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Pipo W4
sensor:modalias:acpi:SMO8500*:dmi:*:bvrV8L_WIN32_CHIPHD_*_DX:*:rvnAMICorporation:rnAptioCRB:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Ployer
#########################################
sensor:modalias:acpi:BMA250E*:dmi:*:svnShenzhenPLOYER*:pnMOMO7W:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

#########################################
# Point of View
#########################################

# The Point of View TAB-P800W does not have its product name filled, so we
# match the entire dmi-alias, assuming that the use of a BMA250E +
# bios-version + bios-date combo is unique
sensor:modalias:acpi:BMA250E*:dmi:bvnAmericanMegatrendsInc.:bvr3BAIR1013:bd08/22/2014:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnAptioCRB:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
sensor:modalias:acpi:BMA250E*:dmi:bvnAmericanMegatrendsInc.:bvr3BAIR1014:bd10/24/2014:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnAptioCRB:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Point of View TAB-P1005W-232 (v2.0)
sensor:modalias:acpi:KIOX000A*:dmi:*:rvnPOV:rnI102A:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Point of View TAB-P1006W-232-3G (v1.0)
sensor:modalias:i2c:bmc150_accel:dmi:bvnINSYDECorp.:*:svnInsyde:pnBayTrail:*:rvn105B:rn0E57:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Predia
#########################################

# Predia Basic tablet, most DMI strings are generic, match on BIOS version
sensor:modalias:acpi:BOSC0200*:dmi:bvnINSYDECorp.:bvrMx.WT107.KUBNGEA*svnInsyde:pnCherryTrail:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Prowise
#########################################
sensor:modalias:acpi:SMO8500*:dmi:*:svnProwise:pnPT301:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Reeder
#########################################

# A8iW-Rev.A
sensor:modalias:acpi:SMO8500*:dmi:*:rvnReeder:rnA8iW-Rev.A:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Schneider
#########################################

# SCT101CTM
sensor:modalias:acpi:BOSC0200*:dmi:bvnAmericanMegatrendsInc.:bvrSCH12i.WJ210Z.KtBJRCA03:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Teclast
#########################################
# Teclast F5
sensor:modalias:acpi:KIOX010A*:dmi:*:svnTECLAST:pnF5:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Teclast F6 Pro (2 sensors)
sensor:modalias:acpi:KIOX010A*:dmi:*:svnTECLAST:pnF6Pro:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1
 ACCEL_LOCATION=display

sensor:modalias:acpi:KIOX020A*:dmi:*:svnTECLAST:pnF6Pro:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1
 ACCEL_LOCATION=base

# Teclast Tbook 11 (E5A6)
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTECLAST:pnTbooK11:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Teclast X4 2-in-1 (G4M6)
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTECLAST:pnX4:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Teclast X80 Plus (H5C5)
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTECLAST:pnDefaultstring:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Teclast X80 Pro (E3E6)
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTECLAST:pnX80Pro:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Teclast X89 (E7ED), "tPAD" is too generic also match on BIOS date
sensor:modalias:acpi:SMO8500*:dmi:*bd12/19/2014:*:rvnTECLAST:rntPAD:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# Teclast X98 Plus I (A5C6), generic DMI strings, match entire dmi modalias inc. bios-date
sensor:modalias:acpi:KIOX000A*:dmi:bvnAmericanMegatrendsInc.:bvr5.011:bd11/03/2015:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnCherryTrailCR:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# Teclast X98 Plus II
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTECLAST:pnX98PlusII:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

#########################################
# Thundersoft
#########################################

# Thundersoft TST168 tablet, generic DMI strings, match entire dmi modalias inc. bios-date
sensor:modalias:acpi:BMA250E*:dmi:bvnAmericanMegatrendsInc.:bvr5.6.5:bd04/15/2014:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnAptioCRB:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

#########################################
# Toshiba
#########################################

# Toshiba Encore WT8-B tablet
sensor:modalias:acpi:INVN6500*:dmi:*:svnTOSHIBA:pnTOSHIBAENCORE2WT8-B:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

# Toshiba Encore WT10A tablet
sensor:modalias:acpi:INVN6500*:dmi:*:svnTOSHIBA:pnTOSHIBAWT10-A-103:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Trekstor
#########################################
sensor:modalias:acpi:BMA250*:dmi:*:bvrTREK.G.WI71C.JGBMRBA*:*:svnInsyde:pnST70416-6:*
sensor:modalias:acpi:BMA250*:dmi:*:bvrTREK.G.WI71C.JGBMRBA*:*:svnTrekStor:pnSurfTabwintron7.0ST70416-6:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1

# SurfTab Wintron 10.1 ST10432-3, generic DMI string, use partial BIOS version match
sensor:modalias:acpi:SMO8500*:dmi:*:bvrWintron.R25M.02.0*:*:svnInsyde:pnBayTrail:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

sensor:modalias:acpi:KIOX000A*:dmi:*:svnTrekStor:pnSurfTabtwin10.1:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, 1

sensor:modalias:acpi:KIOX000A*:dmi:*:svnTREKSTOR*:pnPrimetabS11B:*
sensor:modalias:acpi:KIOX000A*:dmi:*:svnTREKSTOR:pnPrimetabT13B:*
sensor:modalias:acpi:BOSC0200*:dmi:*:svnTrekStor*:pnSurfTabtwin11.6:*
sensor:modalias:acpi:BOSC0200*:dmi:*:svnTrekStor*:pnSurfTabduoW110.1(VT4):*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

# alternative version of Trekstor's SurfTab Twin 11.6
sensor:modalias:acpi:BOSC0200*:dmi:*:bvrTP15-VT5.2.1.3:*:svnTrekStor*:pnSurfTabtwin11.6:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, 1, 0; 0, 0, -1

sensor:modalias:acpi:KIOX010A*:dmi:*:svnTREKSTOR:pnPrimebookC11B:*
sensor:modalias:acpi:KIOX010A*:dmi:*:svnTREKSTOR:pnPRIMEBOOKC11B:*
sensor:modalias:acpi:KIOX010A*:dmi:*:svnTREKSTOR:pnYourbookC11B:*
sensor:modalias:acpi:KIOX010A*:dmi:*:svnTREKSTOR:pnYOURBOOKC11B:*
 ACCEL_MOUNT_MATRIX=-1, 0, 0; 0, -1, 0; 0, 0, -1
 ACCEL_LOCATION=display

sensor:modalias:acpi:KIOX020A*:dmi:*:svnTREKSTOR:pnPrimebookC11B:*
sensor:modalias:acpi:KIOX020A*:dmi:*:svnTREKSTOR:pnPRIMEBOOKC11B:*
sensor:modalias:acpi:KIOX020A*:dmi:*:svnTREKSTOR:pnYourbookC11B:*
sensor:modalias:acpi:KIOX020A*:dmi:*:svnTREKSTOR:pnYOURBOOKC11B:*
 ACCEL_MOUNT_MATRIX=0, 1, 0; 1, 0, 0; 0, 0, 1
 ACCEL_LOCATION=base

#########################################
# Umax
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*:svnUMAX:pnVisionBook10WiPro:*
 ACCEL_MOUNT_MATRIX=1, 0, 0; 0, -1, 0; 0, 0, 1

sensor:modalias:acpi:SMO8500*:dmi:*:svnUMAX:pnVisionBook10WiPlus:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1

#########################################
# Voyo
#########################################
# Voyo Winpad A15
# The Winpad A15 does not have its product name filled, so we
# match the entire dmi-alias, assuming that the use of a SMO8500 +
# bios-version + bios-date combo is unique
sensor:modalias:acpi:SMO8500*:dmi:bvnAmericanMegatrendsInc.:bvr5.6.5:bd11/20/2014:br5.6:svnTobefilledbyO.E.M.:pnTobefilledbyO.E.M.:pvrTobefilledbyO.E.M.:rvnAMICorporation:rnAptioCRB:rvrTobefilledbyO.E.M.:cvnToBeFilledByO.E.M.:ct3:cvrToBeFilledByO.E.M.:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, -1

#########################################
# Wortmann
#########################################
sensor:modalias:acpi:KIOX000A*:dmi:*:svnWortmann_AG:pnTERRA_PAD_1061:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; 1, 0, 0; 0, 0, -1

#########################################
# Yours
#########################################
sensor:modalias:acpi:BMA250E*:dmi:*:svnYOURS:pnY8W81:*
 ACCEL_MOUNT_MATRIX=0, -1, 0; -1, 0, 0; 0, 0, 1
